STARTUP CHECK LIST APPENDICES

Version: 1 July 1998 (ORH) Last Update: June 21th, 2001 (PL)

APPENDIX 1: Check that the Pipeline is running (wg5pl)

There should be - 4 windows (DO, RBS , 2 MIDAS) on lower screen, and - 2 windows (display + graphics) on upper;

The DO window should show that it read the last images taken (day calibrations) In case the pipeline is not working (or in case of doubt): - log out from wg5pl ( [Exit] button ) - log in as pipeline (.5arcsec) - start the DO (mouse menu [Data Flow Applications] [DO] - start the RBS (mouse menu [Data Flow applications][RBS] This will create the 4 +2 windows and start everything (there should be some activity at least on the DO window).

APPENDIX 2: power cycle (CAMAC REBOOT )( inside EMMI Control Room )

Press EMMI interlock Power OFF LEMMI Power OFF CAMAC Power OFF NIM Wait 10 seconds Power ON NIM Wait 15 seconds Power ON CAMAC Wait 30 seconds Power ON LEMMI Release EMMI interlock

APPENDIX 3: wa5tcs, wt5tcs and wemmi REBOOT

WORKSTATION ( under the proper local X term )

Option 1

Check whether Rtap is running then shutdown: Login a operator /etc/shutdown -r -y 0

Option 2

nttReboot.sh Warning: When the three workstations are rebooted, the next order must be followed: 1)wa5tcs, 2)wt5tcs, 3)wemmi

APPENDIX 4: wemmi REBOOT ALL lcu’s ( under wemmi local X term )

nttinsInstallRebootLCUs all Check DATE and TIME in wemmi’s Log Monitor during the LCUs reboot process. ( in case of wrong date, boot LCUs again)

APPENDIX 5: FitsList

On xxx (wemmi if SOFI, wsofi if EMMI or SUSI) : create a window as nttops@wg5ooff [NTT Menu] mouse menu. export DISPLAY=xxx:0.0 Go to the directory where the data are: cd /data/raw/yyyy-mm-dd fitslist -who (get your window’s identifier, and the filename of logsheet). fitslist -e (and edit the file).

fitslist ONTT*fits>/data/raw/dataLog/flLog.xxxxxx fitslist -i

APPENDIX 6: wa5tcs REBOOT ALL lcu’s ( under wa5tcs local X term ) nttInstallRebootLCUs all

APPENDIX 7: wt5tcs REBOOT SOME lcu’s ( under wt5tcs local X term )

nttInstallRebootLCUs lt5alt nttInstallRebootLCUs lt5az nttInstallRebootLCUs lt5ra nttInstallRebootLCUs lt5rb nttInstallRebootLCUs lt5ada nttInstallRebootLCUs lt5adb

APPENDIX 8: Checking Pointing Model ( under wt5tcs local xterm )

ccseiMsg & - Environment: lt5alt

Process: alttrkServer Command: getterm - Environment: lt5az Process: aztrkServer Command: getterm - Environment: lt5ra (rb) Process: rottrkServer Command: getterm

APPENDIX 9: Checking side A M4 position ( under wemmi local xterm )

ccseiMsg & Environment: lemsu Process: suidevServer Command: status mirr4 Command: setup mirr4,name SUSI or SOFI.

APPENDIX 10: Disks Monitor

Create a window as nttastro@wg5ops [ntt xterm] mouse menu. diskMonit

APPENDIX 11: dataSubscriber

In an xterm window logged in as astro, type

dataSubscriber &

then :

program Id : as from schedule or service Observer’s name : as from schedule or service click OK in the Subscription for sercice window click CONFIG in the popup window click ACCEPT in the Subscription for sercice window click START RAW click START RED

APPENDIX 12: FitsList -spy

On wg5off( :

create a window as nttops@wg5ooff [NTT Menu] mouse menu.

cd /data/raw/dataLogs

ll -tr fitslist -spy <last fileof ll -tr>.